

|  |  |
| --- | --- |
|  | **QTY: \_\_\_\_\_\_** |
| [ ]  Rotary Chair[ ]  Rotary Chair large occupant[ ]  Rotary Stool |

[*Link to annex A technical spec from the furniture website*](https://www.gcpedia.gc.ca/wiki/Office_Seating_Supply_Arrangements)

|  |  |  |
| --- | --- | --- |
|  | **Criteria** | **Requirement Choices** |
| **A** | *Headrest* | [ ]  No [ ]  Yes [ ]  No preference  |
| **B** | *Backrest Height* | [ ]  Standard *= height between 450mm (17.7 in.) to 660 mm (25.9 in.)*[ ]  High *= height greater than 660mm (26 in.)*[ ]  No preference |
| **B** | *Backrest Style Preference(s)* |  *Note: style represents overall shape, but the design may vary.* [ ]  No preference [ ]  [ ]  [ ]  [ ]   |
| **C** | *Lumbar Support* | [ ]  Adjustable = *min. 50mm (2 in.) adjustment between 150mm (5.9 in.) to 250mm (9.8 in.) for height* | [ ]  Up/down [ ]  In/out [ ]  In/out & up/down  |
| [ ]  Fixed *= between 150 mm (5.9 in.) to 250 mm (9.8 in.)* |
| [ ]  No preference  |
| **D**  | *Armrests*  | [ ]  Adjustable  | [ ]  height *= HEIGHT: min. 63mm (2.5 in.) adjustment between 176mm (6.9 in.) to 289mm (11.4 in.)*[ ]  height & width *= WIDTH: min.75mm (3 in.) between 443mm (17 in.) to 493mm (19.4 in.)*[ ]  height, width & pivot *= PIVOT: min. 20 degrees inward and min. 10 degrees outward*[ ]  pivot  |
| [ ]  Fixed *= height range between 200 mm (7.9 in.) to 250 mm (9.8 in.)* |
| [ ]  None (no Armrests) |
| **E** | *Seat Depth* | [ ]  Adjustable *= min. 50mm (2 in.) adjustment within the range 420mm (16.5 in.) to 460mm (18.1 in.)* |
| [ ]  Fixed |  [ ]  Shallow *= 380mm (15 in.) to 420mm (16.5 in.)* [ ]  Medium *= greater than 420mm (16.5 in.) to 460mm (18.1 in.)*  [ ]  Deep *= greater than 460mm (18.1 in.)* |
| [ ]  No preference |
| **F**  | *Seat Width* | *Standard rotary chairs and stools have a minimum width of 450mm (17.7in.)* *Large Occupant models have a minimum width of 560mm (22 in.)* |
| **G** | *Seat Height* | *Rotary Chair* | [ ]  Adjustable  | [ ]  Standard *= includes 417mm (16.4 in.) or less to 512mm (20.2in.) or more* [ ]  Low = *includes 376mm (14.8 in.) to 439mm (17.3 in.)* |
| [ ]  Fixed *= between 417mm (16.4 in.) to 512mm (20.2 in.)* |
| *Rotary Stool* | [ ]  Fixed *= must be equal or greater than 670 mm (27.5 in).*[ ]  Adjustable *= must include range from 580mm (23 in.) to 840 mm (33 in.).* |
| **H** | *Tilt Mechanism*  | [ ]  Synchro tilt *= seat and backrest tilt at the same time in a simultaneous movement, with the seat in a ratio greater than 1:1*[ ]  Unison tilt *= Seat and backrest (including knee) tilt in unison, a ratio of 1:1*[ ]  Back tilt *= Seat angle and back angle adjustment to be adjustable independently of each other*[ ]  No preference |
| **I** | *Seat and Backrest Locks* | [ ]  Setup Position *= seat is in the most horizontal position and the backrest in the most vertical position*[ ]  Multiple Positions *= includes the setup position and additional angles of seat and backrest*[ ]  No preference |
| **J** | *Casters* | [ ]  carpet *= for carpeted/ soft floors* [ ]  hard surface *= for hard surfaced floors* |
| **L** | *Foot Ring* | *Standard with stool models only* |
|  | *Upholstery* | Backrest  | [ ]  Upholstery [ ]  Mesh [ ]  Other \_\_\_\_\_\_\_\_\_\_\_\_ |
| Seat  | [ ]  Upholstery [ ]  Mesh [ ]  Other \_\_\_\_\_\_\_\_\_\_\_\_ |
| [ ]  No preference |
|  | *Additional Criteria* | *Add any additional criteria in this section that is not brand specific like additional padding, frame finish, removable armrests, etc.* |

|  |  |
| --- | --- |
| **Side Chair**  | **QTY: \_\_\_\_\_\_** |



[*Link to Annex A technical specifications*](https://www.gcpedia.gc.ca/wiki/Office_Seating_Supply_Arrangements)

|  |  |  |
| --- | --- | --- |
|  | **Criteria** | **Requirement Choices** |
| **B** | *Backrest Height* | *standard with minimum height of 354 mm (13.9 in)*  |
| *Backrest Style Preference(s)* |  *Note: style represents overall shape, but the design may vary.*   [x]  No preference [ ]  [ ]  [ ]  [ ]   |
| **C** | *Lumbar Support* | [ ]  No[ ]  Yes = *between 150 mm (5.9 in.) to 250 mm (9.8 in.)* |
| **D**  | *Armrests*  | [ ]  Fixed *= height range between 200 mm (7.9 in.) to 250 mm (9.8 in.)* |
| [ ]  Adjustable  | [ ]  Height only *= HEIGHT: min. 63mm (2.5 in.) adjustment between 176mm (6.9 in.) to 289mm (11.4 in.)*[ ]  Height & width only *= WIDTH: min.75mm (3 in.) between 443mm (17 in.) to 493mm (19.4 in.)*  |
| [ ]  No Armrest  |
| **E** | *Seat Depth* | [ ]  Fixed |  [ ]  Shallow *= 380mm (15 in.) to 420mm (16.5 in.)* [ ]  Medium *= greater than 420mm (16.5 in.) to 460mm (18.1 in.)* [ ]  Deep *= greater than 460mm (18.1 in.)*[ ]  No preference |
| **F**  | *Seat Width* | *standard with minimum width of 400mm (15.7in.)*  |
| **G** | *Seat Height* | [x]  Fixed *= between 417mm (16.4 in.) to 512mm (20.2 in.)* |
| **H** | *Stacking:* | [ ]  nesting (horizontal stacking) [ ]  (vertical stacking) [ ]  No preference |
| *Base Style* | [ ]  Legs (4 post) | [ ]  Casters [ ]  Glides [ ]  Other: |
| [ ]  Sled [ ]  Cantilever [ ]  Other \_\_\_\_\_\_\_\_\_\_\_[ ]  No preference |
|  | *Upholstery* | Backrest  | [ ]  Upholstery [ ]  Mesh [ ]  Other \_\_\_\_\_\_\_\_\_\_\_\_ |
| Seat  | [ ]  Upholstery [ ]  Mesh [ ]  Other \_\_\_\_\_\_\_\_\_\_\_\_ |
| [ ]  No preference |
|  | *Additional Criteria* | *Add any additional criteria in this section that is not brand specific like additional padding, frame finish, removable armrests , etc.* |