

|  |  |
| --- | --- |
|  | **QTY: \_\_\_\_\_\_** |
| Rotary Chair  Rotary Chair large occupant  Rotary Stool | |

[*Link to annex A technical spec from the furniture website*](https://www.gcpedia.gc.ca/wiki/Office_Seating_Supply_Arrangements)

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | **Criteria** | **Requirement Choices** | | | | |
| **A** | *Headrest* | No  Yes  No preference | | | | |
| **B** | *Backrest Height* | Standard *= height between 450mm (17.7 in.) to 660 mm (25.9 in.)*  High *= height greater than 660mm (26 in.)*  No preference | | | | |
| **B** | *Backrest Style Preference(s)* | *Note: style represents overall shape, but the design may vary.*    No preference | | | | |
| **C** | *Lumbar Support* | Adjustable = *min. 50mm (2 in.) adjustment between 150mm (5.9 in.) to 250mm (9.8 in.) for height* | | | | Up/down  In/out  In/out & up/down |
| Fixed *= between 150 mm (5.9 in.) to 250 mm (9.8 in.)* | | | | |
| No preference | | | | |
| **D** | *Armrests* | Adjustable | | height *= HEIGHT: min. 63mm (2.5 in.) adjustment between 176mm (6.9 in.) to 289mm (11.4 in.)*  height & width *= WIDTH: min.75mm (3 in.) between 443mm (17 in.) to 493mm (19.4 in.)*  height, width & pivot *= PIVOT: min. 20 degrees inward and min. 10 degrees outward*  pivot | | |
| Fixed *= height range between 200 mm (7.9 in.) to 250 mm (9.8 in.)* | | | | |
| None (no Armrests) | | | | |
| **E** | *Seat Depth* | Adjustable *= min. 50mm (2 in.) adjustment within the range 420mm (16.5 in.) to 460mm (18.1 in.)* | | | | |
| Fixed | | Shallow *= 380mm (15 in.) to 420mm (16.5 in.)*  Medium *= greater than 420mm (16.5 in.) to 460mm (18.1 in.)*  Deep *= greater than 460mm (18.1 in.)* | | |
| No preference | | | | |
| **F** | *Seat Width* | *Standard rotary chairs and stools have a minimum width of 450mm (17.7in.)*  *Large Occupant models have a minimum width of 560mm (22 in.)* | | | | |
| **G** | *Seat Height* | *Rotary Chair* | | Adjustable | Standard *= includes 417mm (16.4 in.) or less to 512mm (20.2in.) or more*  Low = *includes 376mm (14.8 in.) to 439mm (17.3 in.)* | |
| Fixed *= between 417mm (16.4 in.) to 512mm (20.2 in.)* | | |
| *Rotary Stool* | | Fixed *= must be equal or greater than 670 mm (27.5 in).*  Adjustable *= must include range from 580mm (23 in.) to 840 mm (33 in.).* | | |
| **H** | *Tilt Mechanism* | Synchro tilt *= seat and backrest tilt at the same time in a simultaneous movement, with the seat in a ratio greater than 1:1*  Unison tilt *= Seat and backrest (including knee) tilt in unison, a ratio of 1:1*  Back tilt *= Seat angle and back angle adjustment to be adjustable independently of each other*  No preference | | | | |
| **I** | *Seat and Backrest Locks* | Setup Position *= seat is in the most horizontal position and the backrest in the most vertical position*  Multiple Positions *= includes the setup position and additional angles of seat and backrest*  No preference | | | | |
| **J** | *Casters* | carpet *= for carpeted/ soft floors*  hard surface *= for hard surfaced floors* | | | | |
| **L** | *Foot Ring* | *Standard with stool models only* | | | | |
|  | *Upholstery* | Backrest | Upholstery  Mesh  Other \_\_\_\_\_\_\_\_\_\_\_\_ | | | |
| Seat | Upholstery  Mesh  Other \_\_\_\_\_\_\_\_\_\_\_\_ | | | |
| No preference | | | | |
|  | *Additional Criteria* | *Add any additional criteria in this section that is not brand specific like additional padding, frame finish, removable armrests, etc.* | | | | |

|  |  |
| --- | --- |
| **Side Chair** | **QTY: \_\_\_\_\_\_** |



[*Link to Annex A technical specifications*](https://www.gcpedia.gc.ca/wiki/Office_Seating_Supply_Arrangements)

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **Criteria** | **Requirement Choices** | | |
| **B** | *Backrest Height* | *standard with minimum height of 354 mm (13.9 in)* | | |
| *Backrest Style Preference(s)* | *Note: style represents overall shape, but the design may vary.*      No preference | | |
| **C** | *Lumbar Support* | No  Yes = *between 150 mm (5.9 in.) to 250 mm (9.8 in.)* | | |
| **D** | *Armrests* | Fixed *= height range between 200 mm (7.9 in.) to 250 mm (9.8 in.)* | | |
| Adjustable | | Height only *= HEIGHT: min. 63mm (2.5 in.) adjustment between 176mm (6.9 in.) to 289mm (11.4 in.)*  Height & width only *= WIDTH: min.75mm (3 in.) between 443mm (17 in.) to 493mm (19.4 in.)* |
| No Armrest | | |
| **E** | *Seat Depth* | Fixed | | Shallow *= 380mm (15 in.) to 420mm (16.5 in.)*  Medium *= greater than 420mm (16.5 in.) to 460mm (18.1 in.)*  Deep *= greater than 460mm (18.1 in.)*  No preference |
| **F** | *Seat Width* | *standard with minimum width of 400mm (15.7in.)* | | |
| **G** | *Seat Height* | Fixed *= between 417mm (16.4 in.) to 512mm (20.2 in.)* | | |
| **H** | *Stacking:* | nesting (horizontal stacking)  (vertical stacking)  No preference | | |
| *Base Style* | Legs (4 post) | | Casters  Glides  Other: |
| Sled  Cantilever  Other \_\_\_\_\_\_\_\_\_\_\_  No preference | | |
|  | *Upholstery* | Backrest | Upholstery  Mesh  Other \_\_\_\_\_\_\_\_\_\_\_\_ | |
| Seat | Upholstery  Mesh  Other \_\_\_\_\_\_\_\_\_\_\_\_ | |
| No preference | | |
|  | *Additional Criteria* | *Add any additional criteria in this section that is not brand specific like additional padding, frame finish, removable armrests , etc.* | | |